          VILLAGE OF CHITTENANGO
"Where the water runs north"
222 GENESEE STREET
CHI'ITENANGO, NEW YORK 13037
PHONE: (315) 687-3936 
www.chittenango.Gov


PUBLIC NOTICE
Village of Chittenango Asphalt Paving Bid Notice
NOTICE IS GIVEN that the Board of Trustees of the Village of Chittenango, County of Madison, in the State of New York solicits bids for asphalt paving including tack coat. Specifications may be obtained via email or mail by contacting the Village Clerk's Office at 222 Genesee St, Chittenango, New York or viewed online at:
https://chittenango.gov/departments/department-of-public-works 
Please contact Village Administrator, Bob Freunscht at (315) 415-7286 or Administrator@Chittenango.org
Sealed bids will be accepted at the Village Clerk's Office, 222 Genesee St, Chittenango, New York, up to 10:00 a.m. on Tuesday, April 21st, 2026 when bids will be opened. In person Bidders may attend the opening at the Clerk's Office or Bidders can contact the Office for results information at (315) 687-3936. The Board of Trustees reserves the right to reject any and all bids received.  Bids must include Non-Collusive Bidding Certification and all Bidders must be on the Public Works Contractor Registry Database.
Winning bid shall provide Village of Chittenango a Certificate of Insurance prior to the start of paving.
Karen M. Hawkins
Village Clerk-Treasurer




VILLAGE OF CHITTENANGO
Paving Project Description 2026-2027 FY

Milling: The Village of Chittenango is responsible for all milling and cleanup.
The contractor shall do the tack coating and paving operations and will also be responsible for the protection of traffic and flagging.
1. Rouse St (Parker to Route 5) 1723’ x 22’
Tack Coat: Prior to paving Rouse, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango. 
Pavinq: Pave the milled area of Rouse using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1723 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
2. Bailey St (Webber to Forbes) 1062’ x 22’ 
Tack Coat: Prior to paving Bailey, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Pavinq: Pave the milled area of Bailey using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1062 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
3. Forbes Ave (Entire Length) 1140’ x 22’
Tack Coat: Prior to paving Forbes, the contractor will apply tack coat to the entire area to be paved, The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of Forbes using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1140 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
4. Charles St (Webber to Forbes) 1082’ x 22’
Tack Coat: Prior to paving Charles, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of Charles using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1082 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
5. Norton Ave (Charles to Warren) 822’ x 22’
Tack Coat: Prior to paving Norton, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of Norton using 1 1/2" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 822 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
6. Cain St (Webber to Norton) 622’ x 22’
Tack Coat: Prior to paving Cain, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of Cain using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 622 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
7. South Berkey (Route 5 to End) 1220’ x 22’
Tack Coat: Prior to paving South Berkey the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of South Berkey using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1220 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.
8. Laura (South Berkey to South Berkey) 1298’ x 22’
Tack Coat: Prior to paving Laura, the contractor will apply tack coat to the entire area to be paved. The application rate for tack coat shall be approximately .05 gallons per square yard. Note: Any final sweeping and/or cleaning will be the responsibility of The Village of Chittenango.
Paving: Pave the milled area of Laura using 1.5" average compacted thickness of Type 7 Top, at a width of approximately 22 ft. wide for 1298 ft. Note: Prior to placing the surface course, it may be necessary to true and level the roadway in areas determined by the Highway Superintendent and the Contractor.

NON-COLLUSIVE BIDDNG CERTIFICATION
Required by Section 139-D of the State Finance Law
By submission of this bid, the Bidder and each person signing on behalf of the Bidder certifies, and in the case of joint bid, each party thereto certifies as to its own organization, under penalty of perjury, that to the best of his/her knowledge and belief:
[I] The prices of this bid have been arrived at independently, without collusion, consultation, communication, or agreement, for the purposes of restricting competition, as to any matter relating to such prices with any other Bidder or with any competitor.
[2] Unless otherwise required by law, the prices which have been quoted in this bid have not been knowingly disclosed by the Bidder and will not knowingly be disclosed by the Bidder prior to opening, directly or indirectly, to any other Bidder or to any competitor; and
[3] No attempt has been made or will be made by the Bidder to induce any other person, partnership or corporation to submit or not to submit a bid for the purpose of restricting competition.
A BID SHALL NOT BE CONSIDERED FOR AWARD NOR SHALL ANY AWARD BE MADE WHERE [1], [2] [3] ABOVE HAVE NOT BEEN COMPLIED WITH; PROVIDED HOWEVER, THAT IF IN ANY CASE THE BIDDER(S) CANNOT MAKE THE FORGOING CERTIFICATION, THE BIDDER SHALL SO STATE AND SHALL FURNISH BELOW A SIGNED STATEMENT WHICH SETS FORTH IN DETAIL FOR THE REASONS THEREFORE:
(AFFIX ADDENDUM TO THIS PAGE IF SPACE IS REQUIRED FOR STATEMENT.]
Subscribed to under penalty of perjury under the laws of the State of New York, this ________ day of _______ , 2026 as the act and deed of said corporation or partnership. 

IF BIDDER(S) (ARE) A PARTNERSHIP, COMPLETE THE FOLLOWING:
NAMES OF PARTNERS OR PRINCIPALS LEGAL RESIDENCE
[image: ]
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[image: ]
[image: ]

IF BIDDER(S) (ARE) A CORPORATION, COMPLETE THE FOLLOWING:

NAMES						LEGAL RESIDENCE

[image: ]
President

[image: ]
Secretary

[image: ]
Treasurer

[image: ]
President

[image: ]
Secretary

[image: ]
Treasurer

Identifying Data:

Potential Contractor: _________________________________________________

Street Address: ___________________________________________________________

City, Town, State, Zip: ________________________________________________

 Telephone: _______________________________________________________________	


If applicable, Responsible Corporate Officer Name


Title


Signature






Joint or combined bids by companies or firms must be certified on behalf of each participant:


[image: ]

Legal name of person, firm or corporation                   Legal name of person, firm or corporation

	
By _______________________________	       By _______________________________
	(Name)	(Name)

________________________________		_______________________________
Title							Title

_________________________________		_______________________________
Street Address 					Street Address

__________________________________		_______________________________
City and State 						City and State
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Page 
	 
image5.jpg




image6.jpg




image7.jpg




image8.jpg




image1.jpeg




image9.jpg




image10.jpg




image11.jpg




image12.jpg




image2.jpg




image3.jpg




image4.jpg




